Bitte auch CMOS Reset durchzuführen:

1.

Shut down the operating system properly, then tu rn off the computer and any external devices, and disconnect the power cord from the power outlet.

2.

With the power cord disconnecte

d, press the power button again to drain the system of any residual power.

3.

Remove the access panel.

4.

Locate the header and jumper labeled CLR\_CMOS on models 3400/3405 or CMOS on model

3410

5.

Remove the jumper from pins 2 and 3.

6.

Place the jumper on pins 1 or 2.

7.

Put the jumper back on pins 2 or 3.

8.

Replace the access panel.

9.

Reconnect the external equipment.

10.

Plug in the computer and turn

on power. Allow the operating syst

em to start. This clears the

current passwords and disabl

es the password features.